By updating a GEN Firmware older than V1.6.0.0. it is very important that you first Update the Bootloader-File. 
After the Bootloader-File was updated successfully, you can perform the update to the new GEN-Firmware.